;DIS_Luminous_Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;DIS_Wattage##ELECTRICAL_WATTAGE##WATTS;DIS_Colour_Temperature##COLOR_TEMPERATURE##KELVIN;DIS_Colour_Rendering_Index_CRI##OTHER##;DIS_Product_Code##OTHER##;DIS_Model##OTHER##;DIS_Photometrics##OTHER##;DIS_Accessories##OTHER##;DIS_Weight##OTHER##;DIS_Insulation_Class##OTHER##;DIS_Dimension##OTHER##;DIS_Luminaire_Colour##OTHER##;DIS_Emergency##OTHER##;DIS_Dimmability##OTHER##;DIS_Emergency_Mode_Operating##OTHER##
143535-00_37W_4093lm_4000K_White;4093;37;4000;80;143535-00;731 Minicomfort LED x4 - UGR16;DIS_731 Minicomfort LED x4 - UGR16 - Photometrics : 731_4x_LED_CLD_CELL_143535-00;;4.67;I;L596xW596xH63;DIS_White;0;0;
143535-12_36W_4093lm_4000K_White;4093;36;4000;80;143535-12;731 Minicomfort LED x4 - UGR16;DIS_731 Minicomfort LED x4 - UGR16 - Photometrics : 731_4x_LED_CLD_CELL-D_143535-12;;4.83;I;L596xW596xH63;DIS_White;0;1;
143535-0041_38W_4093lm_4000K_White;4093;38;4000;80;143535-0041;731 Minicomfort LED x4 - UGR16;DIS_731 Minicomfort LED x4 - UGR16 - Photometrics : 731_4x_LED_CLD_CELL-D-D_143535-0041;;4.7;I;L596xW596xH63;DIS_White;0;1;
143535-9441_37W_4093lm_4000K_White;4093;37;4000;80;143535-9441;731 Minicomfort LED x4 - UGR16;DIS_731 Minicomfort LED x4 - UGR16 - Photometrics : 731_4x_LED_CLD_CELL-D-D-E_143535-9441;;5;I;L596xW596xH63;DIS_White;1;1;1h, the Luminous flux reduces, value available on request.
143535-94_37W_4093lm_4000K_White;4093;37;4000;80;143535-94;731 Minicomfort LED x4 - UGR16;DIS_731 Minicomfort LED x4 - UGR16 - Photometrics : 731_4x_LED_CLD_CELL-D-E_143535-94;;4.78;I;L596xW596xH63;DIS_White;1;1;1h, the Luminous flux reduces, value available on request.
143535-07_37W_4093lm_4000K_White;4093;37;4000;80;143535-07;731 Minicomfort LED x4 - UGR16;DIS_731 Minicomfort LED x4 - UGR16 - Photometrics : 731_4x_LED_CLD_CELL-E_143535-07;;4.9;I;L596xW596xH63;DIS_White;1;0;1h, the Luminous flux reduces, value available on request.
143539-00_37W_3901lm_4000K_White;3901;37;4000;90;143539-00;731 Minicomfort LED x4 - UGR16;DIS_731 Minicomfort LED x4 - UGR16 - Photometrics : 731_4xled_cri90_CLD_CELL_143539-00;;4.64;I;L596xW596xH63;DIS_White;0;0;
143539-12_37W_3901lm_4000K_White;3901;37;4000;90;143539-12;731 Minicomfort LED x4 - UGR16;DIS_731 Minicomfort LED x4 - UGR16 - Photometrics : 731_4xled_cri90_CLD_CELL-D_143539-12;;4.83;I;L596xW596xH63;DIS_White;0;1;
143539-0041_37W_3901lm_4000K_White;3901;37;4000;90;143539-0041;731 Minicomfort LED x4 - UGR16;DIS_731 Minicomfort LED x4 - UGR16 - Photometrics : 731_4xled_cri90_CLD_CELL-D-D_143539-0041;;4.7;I;L596xW596xH63;DIS_White;0;1;
143539-9441_37W_3901lm_4000K_White;3901;37;4000;90;143539-9441;731 Minicomfort LED x4 - UGR16;DIS_731 Minicomfort LED x4 - UGR16 - Photometrics : 731_4xled_cri90_CLD_CELL-D-D-E_143539-9441;;5;I;L596xW596xH63;DIS_White;1;1;1h, the Luminous flux reduces, value available on request.
143539-94_37W_3901lm_4000K_White;3901;37;4000;90;143539-94;731 Minicomfort LED x4 - UGR16;DIS_731 Minicomfort LED x4 - UGR16 - Photometrics : 731_4xled_cri90_CLD_CELL-D-E_143539-94;;4.78;I;L596xW596xH63;DIS_White;1;1;1h, the Luminous flux reduces, value available on request.
143539-07_37W_3901lm_4000K_White;3901;37;4000;90;143539-07;731 Minicomfort LED x4 - UGR16;DIS_731 Minicomfort LED x4 - UGR16 - Photometrics : 731_4xled_cri90_CLD_CELL-E_143539-07;;4.9;I;L596xW596xH63;DIS_White;1;0;1h, the Luminous flux reduces, value available on request.
