;DIS_Luminous_Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;DIS_Wattage##ELECTRICAL_WATTAGE##WATTS;DIS_Colour_Temperature##COLOR_TEMPERATURE##KELVIN;DIS_Colour_Rendering_Index_CRI##OTHER##;DIS_Product_Code##OTHER##;DIS_Model##OTHER##;DIS_Photometrics##OTHER##;DIS_Accessories##OTHER##;DIS_Weight##OTHER##;DIS_Insulation_Class##OTHER##;DIS_Dimension##OTHER##;DIS_Luminaire_Colour##OTHER##;DIS_Emergency##OTHER##;DIS_Dimmability##OTHER##;DIS_Emergency_Mode_Operating##OTHER##
153533-00_37W_4093lm_4000K_White;4093;37;4000;80;153533-00;841 Minicomfort LED R x2 - UGR16;DIS_841 Minicomfort LED R - UGR16 - Photometrics : 841_led_R_CLD_CELL_153533-00;;2.91;I;L1196xW294xH60;DIS_White;0;0;
153533-12_37W_4093lm_4000K_White;4093;37;4000;80;153533-12;841 Minicomfort LED R x2 - UGR16;DIS_841 Minicomfort LED R - UGR16 - Photometrics : 841_led_R_CLD_CELL-D_153533-12;;2.69;I;L1196xW294xH60;DIS_White;0;1;
153533-0041_38W_4093lm_4000K_White;4093;38;4000;80;153533-0041;841 Minicomfort LED R x2 - UGR16;DIS_841 Minicomfort LED R - UGR16 - Photometrics : 841_led_R_CLD_CELL-D-D_153533-0041;;2.21;I;L1196xW294xH60;DIS_White;0;1;
153533-9441_33W_4093lm_4000K_White;4093;33;4000;80;153533-9441;841 Minicomfort LED R x2 - UGR16;DIS_841 Minicomfort LED R - UGR16 - Photometrics : 841_led_R_CLD_CELL-D-D-E_153533-9441;;3.67;I;L1196xW294xH60;DIS_White;1;1;1h, the Luminous flux reduces, value available on request.
153533-94_36W_4093lm_4000K_White;4093;36;4000;80;153533-94;841 Minicomfort LED R x2 - UGR16;DIS_841 Minicomfort LED R - UGR16 - Photometrics : 841_led_R_CLD_CELL-D-E_153533-94;;2.68;I;L1196xW294xH60;DIS_White;1;1;1h, the Luminous flux reduces, value available on request.
153533-07_37W_4093lm_4000K_White;4093;37;4000;80;153533-07;841 Minicomfort LED R x2 - UGR16;DIS_841 Minicomfort LED R - UGR16 - Photometrics : 841_led_R_CLD_CELL-E_153533-07;;3.21;I;L1196xW294xH60;DIS_White;1;0;1h, the Luminous flux reduces, value available on request.
