;DIS_Luminous_Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;DIS_Wattage##ELECTRICAL_WATTAGE##WATTS;DIS_Colour_Temperature##COLOR_TEMPERATURE##KELVIN;DIS_Colour_Rendering_Index_CRI##OTHER##;DIS_Product_Code##OTHER##;DIS_Model##OTHER##;DIS_Photometrics##OTHER##;DIS_Accessories##OTHER##;DIS_Weight##OTHER##;DIS_Insulation_Class##OTHER##;DIS_Dimension##OTHER##;DIS_Luminaire_Colour##OTHER##;DIS_Emergency##OTHER##;DIS_Dimmability##OTHER##;DIS_Emergency_Mode_Operating##OTHER##
153535-00_28W_4093lm_4000K_White;4093;37;4000;80;153535-00;841 Minicomfort LED x4 - UGR16;DIS_841 Minicomfort LED x4 - UGR16 - Photometrics : 841_4x_led_CLD_CELL_153535-00;;2.91;I;L596xW596xH60;DIS_White;0;0;
153535-12_27W_4093lm_4000K_White;4093;37;4000;80;153535-12;841 Minicomfort LED x4 - UGR16;DIS_841 Minicomfort LED x4 - UGR16 - Photometrics : 841_4x_led_CLD_CELL-D_153535-12;;2.91;I;L596xW596xH60;DIS_White;0;1;
153535-0041_28W_4093lm_4000K_White;4093;38;4000;80;153535-0041;841 Minicomfort LED x4 - UGR16;DIS_841 Minicomfort LED x4 - UGR16 - Photometrics : 841_4x_led_CLD_CELL-D-D_153535-0041;;2.91;I;L596xW596xH60;DIS_White;0;1;
153535-9441_27W_4093lm_4000K_White;4093;37;4000;80;153535-9441;841 Minicomfort LED x4 - UGR16;DIS_841 Minicomfort LED x4 - UGR16 - Photometrics : 841_4x_led_CLD_CELL-D-D-E_153535-9441;;2.91;I;L596xW596xH60;DIS_White;1;1;1h, the Luminous flux reduces, value available on request.
153535-94_27W_4093lm_4000K_White;4093;37;4000;80;153535-94;841 Minicomfort LED x4 - UGR16;DIS_841 Minicomfort LED x4 - UGR16 - Photometrics : 841_4x_led_CLD_CELL-D-E_153535-94;;3.49;I;L596xW596xH60;DIS_White;1;1;1h, the Luminous flux reduces, value available on request.
153535-07_31W_4093lm_4000K_White;4093;40;4000;80;153535-07;841 Minicomfort LED x4 - UGR16;DIS_841 Minicomfort LED x4 - UGR16 - Photometrics : 841_4x_led_CLD_CELL-E_153535-07;;3.91;I;L596xW596xH60;DIS_White;1;0;1h, the Luminous flux reduces, value available on request.
153539-00_37W_3901lm_4000K_White;3901;37;4000;90;153539-00;841 Minicomfort LED x4 - UGR16;DIS_841 Minicomfort LED x4 - UGR16 - Photometrics : 841_4xled_cri90_CLD_CELL_153539-00;;2.85;I;L596xW596xH60;DIS_White;0;0;
153539-12_37W_3901lm_4000K_White;3901;37;4000;90;153539-12;841 Minicomfort LED x4 - UGR16;DIS_841 Minicomfort LED x4 - UGR16 - Photometrics : 841_4xled_cri90_CLD_CELL-D_153539-12;;2.91;I;L596xW596xH60;DIS_White;0;1;
153539-0041_37W_3901lm_4000K_White;3901;37;4000;90;153539-0041;841 Minicomfort LED x4 - UGR16;DIS_841 Minicomfort LED x4 - UGR16 - Photometrics : 841_4xled_cri90_CLD_CELL-D-D_153539-0041;;3.05;I;L596xW596xH60;DIS_White;0;1;
153539-9441_37W_3901lm_4000K_White;3901;37;4000;90;153539-9441;841 Minicomfort LED x4 - UGR16;DIS_841 Minicomfort LED x4 - UGR16 - Photometrics : 841_4xled_cri90_CLD_CELL-D-D-E_153539-9441;;2.91;I;L596xW596xH60;DIS_White;1;1;1h, the Luminous flux reduces, value available on request.
153539-94_37W_3901lm_4000K_White;3901;37;4000;90;153539-94;841 Minicomfort LED x4 - UGR16;DIS_841 Minicomfort LED x4 - UGR16 - Photometrics : 841_4xled_cri90_CLD_CELL-D-E_153539-94;;3.49;I;L596xW596xH60;DIS_White;1;1;1h, the Luminous flux reduces, value available on request.
153539-07_37W_3901lm_4000K_White;3901;37;4000;90;153539-07;841 Minicomfort LED x4 - UGR16;DIS_841 Minicomfort LED x4 - UGR16 - Photometrics : 841_4xled_cri90_CLD_CELL-E_153539-07;;3.91;I;L596xW596xH60;DIS_White;1;0;1h, the Luminous flux reduces, value available on request.
